LIMITED FIVE-YEAR WARRANTY
North Coast Cultured Products, Inc. warrants this product to be free of manufactured defects.  North Coast Cultured Products, Inc. will at its election, repair, replace or make appropriate pro-rated adjustment where North Coast Cultured Products, Inc. inspection discloses any such defects occurring in normal usage within five years from date of purchase.  

This warranty does not cover removal or reinstallation charges of any product supplied by North Coast Cultured Products, Inc. and is also not applicable to the following:
1.	Any product installed or used in a manner contrary to normal recommended usage.
2.	Damages to the product while in transit or during installation by third party
3.	Cracks or chips on surfaces of product unless caused by defects in workmanship or material.
4.	Slight imperfections, non-uniform patterns, warping & bowing, color variations, and other conditions commonly found in products of nature such as stone and quarried material.

This warranty is in lieu of all warranties including warranties of merchantability and fitness for a particular purpose except any applicable warranties, and as to such implied warranties, its obligation shall be limited to conditions covered by the warranty which occur within five (5) years from the consumer’s purchase of the product.  In no event shall North Coast Cultured Product Products, Inc be liable for incidental or consequential damages which may result from any defect in the product or breach of this warranty.

Under the terms of this warranty, the purchaser will be required to bear the cost of removal and reinstallation of any transportation costs or cartage charges to return the product to our plant. 
WARNING
Use of PLUMBERS PUTTY on drain will void warranty.

INSTALLER
Apply 100% Silicone to underside of drain collar.  Be sure to use bottom rubber washer and metal washer.  Tighten to Finger Tightness.  Then turn one full turn with wrench to seal.  Not Responsible for Bowl Cracking Due to Excessive Pull Down On Drain Plug.

AFORDABLE ELEGANCE

    

580 Mayer Street
Building #7
Bridgeville, PA  15017

Phone: (412) 206~0008	Fax: (412) 206~0036
Toll Free: 1~877~283~7422

Visit us on the Web
Installation Instructions
www.northcoastmarble.com

READ PRIOR TO INSTALLATION

CARE & CLEANING INSTRUCTIONS

IMPORTANT  INSTRUCTIONS  FOR  THE  CARE  AND  CLEANING  OF  NORTH  COAST  CULTURED  PRODUCTS
INSTALLER: PLEASE GIVE THIS TO THE BUILDER OR HOMEOWNER

All North Coast Cultured Products are created individually to fit your needs by skilled craftsmen. Each product is manufactured using premium quality material.  Our care and high standards are visible in the long-lasting beauty of every creation that North Coast Cultured Products produces.  You can protect the splendor and ensure a long life of uncomplicated service from the product by observing these simple suggestions.

•	Never run straight hot water into the basin as this can cause hair-line cracks.  For added safety, keep hot water thermostat at 150 degrees. F or below
•	Tape residue left from labels can be removed by using paste wax and elbow grease.
•	Preserve the luster of your North Coast Cultured Product by occasionally cleaning and waxing.  Use only liquid, non-abrasive cleaners.  Afterward, apply a light coat of non-yellowing wax and polish.
•	Remove hard water scale and rust stains with a mild vinegar and water solution followed by a white fine automobile polishing compound.

Many difficult stains can be avoided by attention to proper use of your North Coast Cultured Product.  These steps can be taken to remedy unusual cleaning problems.

•	Grease stains and oil residues can be removed by kerosene, mineral spirits or butyl-cello solve available from paint outlets.
•	Mold and mildew can be removed with a dilute solution of Clorox or Lysol.   
•	Never let pure Clorox come in contact with your North Coast Cultured Product
•	Hair dye or shoe polish stains can also be removed by using polishing compound.
•	Minor surface scratches can be buffed out using the polishing compound.
•	Deeper scratches can or burns require light sanding with wet 600 grit sandpaper.  Sand lightly with a circular motion in as confined an area as possible, wet area thoroughly while sanding 
•	Remove the minor scratches which result from sanding by buffing with polish compound.
•	Cigarette stains can be removed using Bon Ami applied with a soft toothbrush.  After removing the stain, polish out the area with toothpaste.
•	Small chips can be repaired by applying clear fingernail polish. Then follow the instructions for sanding out scratches.

Certain chemical substances can seriously discolor your product even during brief periods of contact.  Protect your North Coast Cultured Product from contact with these harmful reagents:

•	Clorox and other Hypochlorite bleaches
•	Hydrogen Peroxide in any concentration
•	Drano or other Lye solutions
•	Sani-flush or other Sodium Bisulphate compound
•	Fingernail polish remover
•	Paint Strippers containing Methylene Chloride
•	Comet, Ajax or any other abrasive cleaners

ONLY USE NON-ABRASIVE CLEANERS

We strongly recommend using 

WEIMANS GRANITE AND STONE

Cultured products share the contraction and expansion characteristics of natural marble, granite, stone and onyx.  Attention to temperature change is particularly important during winter months when the temperature of the hot water coming from your hot water tank, and the temperature of the cold-water lines feeding your house is the greatest.  Avoid running hot water exclusively in your sink.  Rapid changes in water temperature can cause it to crack.  Your product should last a lifetime if you turn the temperature in your water heater to the low or mid-range.

Your North Coast Cultured Product is a quality benchmark in the cultured product industry.  With a minimum amount of care, you will be pleased with your purchase for many years.  You can be proud that your product is made by
 NORTH COAST CULTURED PRODUCTS.